# **DHT11**

# [dht.h](https://github.com/adafruit/DHT-sensor-library)

Faz a conversão da leitura analogica do sensor para graus celsius e/ou fahrenheit

# **DS18B20**

* [OneWire.h](https://github.com/PaulStoffregen/OneWire)
* [dallasTemperature.h](https://www.arduino.cc/reference/en/libraries/dallastemperature/)

# **MQTT**

# [PubSubClient.h](https://github.com/knolleary/pubsubclient/releases/tag/v2.8)

# 

# **WIFI**

# [WiFi.h](https://github.com/khoih-prog/WebServer_ESP32_ENC)

# [WiFiManager.h](https://github.com/tzapu/WiFiManager)

# 

# **DEEP\_SLEEP**

* [neotimer.h](https://github.com/jrullan/neotimer)